# DMA-Flash-Tools
## How To Use
Insert the DMA board's jtag/uart port and put your firmware in "flash tools", then run script on the secondary machine
![image](https://github.com/kilmu1337/DMA-Flash-Tools/assets/155318836/dc46de01-4af4-45e2-9826-746bbf851658)


> [!NOTE]
>
> I'm happy to help you. Please cite the source if you share this script.

Website: [https://kilmu.dev/](https://kilmu.dev/)

Discord Channel: https://discord.gg/KilmuDMA








